Watch keep updating the time for every minute until watch turn off

Convert the data to watch binary time settings and save to a non-volatile filesystem (preferences.h)

Get the data using Wi-Fi connection (multi connection network environment using async TCP library)

Set time and color settings in the page and sync the data

Direct to control settings webpage

NO

Direct to SSID and password reset form and update the user credential

YES

Check, Is that a default SSID and password?

Direct to default IP address

Connect to the watch’s hotspot using phone or PC